For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Auxiliary Heater Pump Nut | 10 N·m | 89 lb in
Cooling Fan Control Switch | 22 N·m | 16 lb ft
Engine Coolant Crossover Bolt | 30 N·m | 22 lb ft
Engine Coolant Heater | 60 N·m | 44 lb ft
Engine Coolant Intake Pipe Bolt | 20 N·m | 15 lb ft
Engine Coolant Intake Pipe Support Bolt | 20 N·m | 15 lb ft
Engine Coolant Temperature Sender | 20 N·m | 15 lb ft
Engine Splash Shield Bolt | 10 N·m | 89 lb in
Oil Cooler Outlet Line to the Engine Block | 30 N·m | 22 lb ft
Oil Cooler Outlet Line to the Oil Cooler Cover | 30 N·m | 22 lb ft
Power Steering Reservoir Bracket Bolt | 7 N·m | 62 lb in
Primary Engine Cooling Fan Housing-to-Radiator | 4 N·m | 35 lb in
Primary Engine Cooling Fan Motor-to-Housing Nut | 4 N·m | 35 lb in
Secondary AIR Cut-Off Valve Bracket | 4 N·m | 35 lb in
Thermostat Housing Bolt | 20 N·m | 15 lb ft
Thermostat Outlet Pipe Bolt | 20 N·m | 15 lb ft
Transmission Oil Cooler Bolt | 25 N·m | 18 lb ft
Water Pump Bolts | 25 N·m | 18 lb ft
Water Pump Pulley Bolt | 10 N·m | 89 lb in