For 1990-2009 cars

### Removal Procedure

1. Remove the trim panel. Refer to Front Side Door Trim Panel Replacement .
2. Remove the retaining block.

Use a pair of pliers to remove the center wedge pin.

### Installation Procedure

1. Install the retaining block:

• | Push the block into the door.

• | Push the center wedge into place using a screwdriver.

2. Install the trim panel. Refer to Front Side Door Trim Panel Replacement .