For 1990-2009 cars

### Removal Procedure

#### Tools Required

J 42081 Door Hinge Pin Remover and Installer

1. Disable the SIR system If equipped with the SIR side impact system. Refer to Disabling the SIR System .
2. Tape the edges of the door and the fender in order to prevent damage when removing.
3. Remove the rubber conduit. Refer to Front Side Door Conduit Replacement .
4. Disconnect the front door electrical connectors to the door.
5. Remove the wiring harness from the front pillar.
6. Support the door with a suitable stand.
7. Remove the check link. Refer to Front Side Door Check Link Replacement .
8. Remove the hinge pins using the J 42081.
9. Remove the weather caps from the pins.
10. Insert the J 42081 around the hinge collar while tapping each pin lightly with a hammer until the hinge pin release.
11. Remove the door with the aid of a assistant.

### Installation Procedure

1. Install the door with aid of a assistant.
2. Install the hinge pins:

• | Insert the J 42081 around the hinge collar while using a small hammer to tap each pin into the hinge hole.

• | Install the weather caps.

3. Remove the door support.
4. Inspect the door to body alignment.
5. Install the check link. Refer to Front Side Door Check Link Replacement .
6. Install the front pillar wiring harness.
7. Connect all electrical connectors that were removed.
8. Install the rubber conduit. Refer to Front Side Door Conduit Replacement .
9. Remove the tape from the door and the fender.
10. Enable the SIR system If equipped with the SIR side impact system. Refer to Enabling the SIR System .