For 1990-2009 cars

Important: The steps outlined in this procedure are general requirements for properly setting the rear toe.

The alignment equipment varies in design and capabilities, therefore, consult with the equipment manufacturer's guidelines prior to setting this angle.
1. Loosen both tie rod adjuster clamps.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Turn the threaded sleeve until you achieve the desired toe specification.

Tighten
Tighten the tie rod adjuster clamp bolts to 15 N·m (11 lb ft).