For 1990-2009 cars

### Removal Procedure

Important: Always replace the cables and the rear guide in pairs.

1. Remove the sunroof actuator. Refer to Sunroof Actuator Replacement
2. Remove the water gutter. Refer to Water Gutter Replacement
3. Remove the screw from the sunroof actuator cable stop.
4. Remove the sunroof actuator cable stop from the sunroof actuator.
5. Remove the slide and/or guide from the sunroof actuator.
6. Remove the pin and C-clip.
7. Disconnect the cable and the rear guide from the slide.

### Installing Procedure

1. Install the cable and the rear guide to the slide. Sparingly lubricate cables, use Silicon Grease, GM P/N 12345579 or equivalent.
2. Install the pin and C-clip.
3. Install the slide and/or guide to the sunroof actuator.
4. Install the sunroof actuator stop to the sunroof actuator.
5. Install the screw to the cable stop sunroof actuator.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

Tighten
Tighten the sunroof actuator cable stop screw until fully seated and no stripped.

6. Install the water gutter. Refer to Water Gutter Replacement
7. Install the sunroof actuator. Refer to Sunroof Actuator Replacement in this section.
8. Adjust both cables with the slide and/or the guide. Refer to Slider Adjustment