For 1990-2009 cars

### Removal Procedure

1. Remove door trim panel. Refer to Rear Side Door Trim Panel Replacement .
2. Remove the trim panel retaining block. Refer to Rear Side Door Trim Panel Bracket Replacement .
3. Pull on the water deflector in order to remove from the door edges.

### Installation Procedure

1. Install the water deflector while rubbing around the edges.
2. Install the trim panel retaining block. Refer to Rear Side Door Trim Panel Bracket Replacement .
3. Install door trim panel. Refer to Rear Side Door Trim Panel Replacement .