For 1990-2009 cars

## Headlamp Bulb Replacement Halogen Headlamp

### Removal Procedure- Halogen Bulb

1. Open the hood.
2. Remove the headlamp capsule from the vehicle. Refer to Headlamp Capsule Replacement .
3. Remove the access cover from the headlamp capsule.
4. Compress and lift the headlamp bulb fastening tangs.
5. Disconnect the electrical connection from the headlamp bulb.

Remove the headlamp bulb from the headlamp capsule.

### Installation Procedure

1. Install the headlamp bulb to the headlamp capsule.

Connect the electrical connection to the headlamp bulb.

2. Compress and install the headlamp bulb fastening tangs.
3. Install the access cover to the headlamp capsule.
4. Install the headlamp capsule to the vehicle. Refer to Headlamp Capsule Replacement .
5. Close the hood.

## Headlamp Bulb Replacement HID Headlamp Sport Model

### Removal Procedure- HID Headlamp Bulb

Caution: The high intensity discharge system produces high voltage and current. To reduce the risk of severe shocks and burns:

• | Never open the high intensity discharge system ballast or the arc tube assembly starter.

• | Never probe between the high intensity discharge system ballast output connector and the arc tube assembly.

Caution: The high intensity discharge system produces high voltage and current. In order to reduce the risk of severe shocks and burns, the battery negative cable must be disconnected any time service work is being performed on or around the high intensity discharge system.

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Remove the headlamp capsule. Refer to Headlamp Capsule Replacement .
3. Remove the three TORX bolts from the lamp cover cap (1).
4. Slide the lamp cover cap with the high voltage cable grommet (4) away from the lamp socket.
5. Remove the high voltage plug (3) by turning to the left and disconnecting.
6. Remove the Xenon lamp fastening ring (5) by turning to the left and remove from the Xenon bulb.
7. Remove the Xenon bulb (6) from the headlamp capsule.

### Installation Procedure

1. Install the Xenon bulb (6) to the headlamp capsule.
2. Install the Xenon lamp fastening ring (5) to the Xenon bulb and turning to the right .
3. Reconnect the high voltage plug (3) and turn to the right.
4. Slide the lamp cover cap with the high voltage cable grommet (4) to the lamp socket.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

5. Install the three TORX bolts to the lamp cover cap (1).

Tighten
Tighten the three TORX bolts to 1.7 N·m (15 lb in).

6. Install the headlamp capsule to the vehicle. Refer to Headlamp Capsule Replacement .
7. Connect the battery negative cable. Refer to Battery Negative Cable Disconnect/Connect Procedure in Engine Electrical.