For 1990-2009 cars

#### Tools Required

J 42072 Rear Brake Backing Plate Bolt Remover

### Removal Procedure

1. Remove the wheel bearing hub. Refer to Rear Wheel Bearing and Hub Replacement in Rear Suspension.
2. Remove the parking brake shoes with the related hardware. Refer to Parking Brake Shoe Replacement .
3. Use the J 42072 to remove the backing plate bolts (1) from the brake backing plate (2).
4. Remove the parking brake anchor (3) from the brake backing plate (2).
5. Remove the brake backing plate (2) from the axle control arm (1).

### Installation Procedure

1. Install the park brake shoe retaining pins, if removed.
2. Install the brake backing plate (2) to the axle control arm (1).
3. Install the parking brake anchor (3) to the brake backing plate (2).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Use theJ 42072 to install the backing plate bolts (1) to the brake backing plate (2).

Tighten
Tighten the backing plate bolts to 50 N·m (37 lb ft).

5. Install the parking brake shoes with the related hardware. Refer to Parking Brake Shoe Replacement .
6. Install the wheel bearing hub. Refer to Rear Wheel Bearing and Hub Replacement in Rear Suspension.
7. Test the parking brake operation. Refer to Parking Brake Lever Adjustment .