For 1990-2009 cars

### Removal Procedure

1. Remove the instrument cluster. Refer to Instrument Cluster Replacement .
2. Remove the screws from the voltage/oil pressure gauge module.
3. Remove the voltage/oil pressure gauge module from the lens by pulling the locking the tabs back and lifting.

### Installation Procedure

1. Install the voltage/oil pressure gauge module to the lens.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the screws to voltage/oil pressure gauge module.

Tighten
Tighten the screws until fully seated but not stripped.

3. Install the instrument cluster. Refer to Instrument Cluster Replacement