For 1990-2009 cars

### Removal Procedure

1. Remove the dome and reading lamp by inserting a flat-bladed screwdriver to the back edge and push downward to release the dome lamp.
2. Remove the electrical connection from the dome lamp.
3. Remove the bulb from the dome lamp.

### Installation Procedure

1. Install the bulb to the dome lamp.
2. Install the electrical connections to the dome lamp.
3. Install the dome and reading front edge in first and snap into place.