For 1990-2009 cars

### Removal Procedure

Caution: When working with any type of glass or sheet metal with exposed or rough edges, wear approved safety glasses and gloves in order to reduce the chance of personal injury.

The rear window reveal molding is pressed into a two piece retainer. The reveal molding retainer is attached to the rear window by a thin bead of butyl tape that is in the groove of the retainer.

1. Carefully pry the end of the rear window reveal molding (1) out of the reveal molding retainers (2) near the base of the rear window.
2. Pull the rear window reveal molding (1) upward and away from the reveal molding retainer and rear window to remove the rear window reveal moldings (1).

### Installation Procedure

1. Insert the rear window reveal molding (1) starting at the upper corners.
2. Working the window reveal molding (1) downward and across to install the rear window reveal moldings.