For 1990-2009 cars

### Removal Procedure

1. Remove the ashtray.
2. Remove the door assist handle molding screw.
3. Remove the door assist handle molding.
4. Remove the door panel. Refer to Rear Side Door Trim Panel Replacement .
5. Disconnect the actuating rod from the door latch.
6. Slide the door assist handle forward.
7. Remove the door assist handle.

### Installation Procedure

1. Install the door assist handle to the door.
2. Connect the actuating rod to the door latch.
3. Install the door panel. Refer to Rear Side Door Trim Panel Replacement .
4. Install the door assist handle molding.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

5. Install the door assist handle screw.

Tighten
Tighten the screw to 20 N·m (15 lb ft).

6. Install the ashtray.
7. Verify the door operation.