For 1990-2009 cars

### Removal Procedure

1. Open the hood.
2. Unscrew the self-locking tab on the RH/and or LH side of the radiator cover.
3. Remove the front turn signal lamp socket from the headlamp.
4. Remove the bulb from the socket.

### Installation Procedure

1. Install the bulb to the socket.
2. Install the socket to the headlamp.
3. Install the RH/and or LH side of the radiator cover.
4. Close the hood.