For 1990-2009 cars

### Removal Procedure

1. Remove the rear parking brake lever. Refer to Park Brake Lever Assembly Replacement .
2. Remove the rear parking brake switch bolt (1) attaching the rear parking brake indicator switch (2) to the lever.
3. Remove the rear parking brake switch wiring harness connector (1) from the rear parking brake switch (2).

### Installation Procedure

1. Install the rear parking brake switch wiring harness connector (1) from the rear parking brake switch (2).
2. Install the rear parking brake switch to the lever.
3. Install the rear parking brake switch bolt (1) attaching the rear parking brake indicator switch (2) to the lever.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

Tighten
Tighten the rear parking brake switch bolt (1) to 3 N·m (27 lb in).

4. Install the rear parking brake lever. Refer to Park Brake Lever Assembly Replacement .