For 1990-2009 cars

### Removal Procedure

1. Open the hood.
2. Remove the grille screws from the grille.
3. Remove the grille from the hood.

### Installation Procedure

1. Position the grille to the hood.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the grille screws to the grille.

Tighten
Tighten the grille screws to 2 N·m (18 lb in).

3. Close the hood.