For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the rear fascia. Refer to Rear Bumper Fascia Replacement .
3. Remove the rear bumper impact bar. Refer to Rear Bumper Impact Bar Replacement
4. Remove the rear bumper fasica support from the impact bar.

### Installation Procedure

1. Install the rear bumper fasica support over the impact bar.
2. Install the rear bumper impact bar. Refer to Rear Bumper Impact Bar Replacement .
3. Install the rear fascia. Refer to Rear Bumper Fascia Replacement .
4. Lower the vehicle.