For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Accelerator Pedal Position Sensor | 22 N·m | 16 lb ft
Air Intake Duct | 3 N·m | 27 lb in
AIR Pipe to Manifold | 20 N·m | 15 lb ft
Camshaft Position Sensor | 8 N·m | 71 lb in
Coil Pack | 8 N·m | 71 lb in
Crankshaft Position Sensor | 8 N·m | 71 lb in
ECT Sensor | 20 N·m | 15 lb ft
EVAP Canister Purge Valve | 12 N·m | 106 lb in
EVAP Vent Solenoid Bracket | 12 N·m | 106 lb in
Fuel Rail Supply and Return Fittings | 15 N·m | 11 lb ft
Fuel Sender Locking Nut | 50 N·m | 37 lb ft
Fuel Tank Pressure Sensor | 8 N·m | 71 lb in
Fuel Tank Retaining Strap | 34 N·m | 25 lb ft
In-Line Fuel Filter Bracket | 10 N·m | 89 lb in
Knock Sensor | 22 N·m | 16 lb ft
MAF Sensor (Clamps) | 8 N·m | 71 lb in
Oxygen Sensor | 41 N·m | 30 lb ft
Throttle Body Bolts | 22 N·m | 16 lb ft