For 1990-2009 cars

### Removal Procedure

1. Disable the SIR system, if equipped with the inflatable restraint side impact system. Refer to Disabling the SIR System in Restraints.
2. Remove the front door trim panel. Refer to Front Side Door Trim Panel Replacement .
3. Remove the water deflector. Refer to Front Side Door Water Deflector Replacement .
4. Slide the inside door handle forward.
5. Turn the handle downward to disegage from the door.
6. Remove the linkage from the handle.

### Installation Procedure

1. Install the handle linkage.
2. Slide the handle rearward in order to lock into place.
3. Install the water deflector. Refer to Front Side Door Water Deflector Replacement .
4. Install the front door trim panel. Refer to Front Side Door Trim Panel Replacement .
5. Enable the SIR system, if equipped with the inflatable restraint side impact system. Refer to Enabling the SIR System in Restraints.