For 1990-2009 cars

#### Tools Required

• | J 21474-5 Bushing Receiver

• | J 21474-18 3/8 Inch Nut

• | J 21474-19 3/8 Inch Bolt

• | J 42092 Front Lower Control Arm Horizontal Bushing Remover/Installer kit

• | J 42112-4 Rear Differential Remover/Installer Tool

• | J 42200 Rear Lower Control Arm Bushing Remover/Installer Bolt

### Removal Procedure

Caution: To avoid any vehicle damage, serious personal injury or death when major components are removed from the vehicle and the vehicle is supported by a hoist, support the vehicle with jack stands at the opposite end from which the components are being removed and strap the vehicle to the hoist.

1. Remove the lower control arm. Refer to Lower Control Arm Replacement
2. Position the J 42092-1 and position the J 42092-2.
3. Press out the horizontal bushing.
4. Position the J 21474-18 , J 21474-5 , J 42112-4 and position the J 21474-19 .
5. Press out the vertical bushing.

### Installation Procedure

1. Position the J 21474-18 ,J 21474-5 , and position the J 21474-19 .
2. Press the vertical bushing into the lower control arm until flush.
3. Position the J 42091-1 and position the J 42092-2.
4. Press the horizontal bushing into the lower control until flush.
5. Install the lower control arm. Refer to Lower Control Arm Replacement

.