For 1990-2009 cars

### Tools Required

• | J 38588-1 Guide Pins

• | J 23082-A Oil Pump Aligner

• | J 36850 Transjel®

1. Install the adapter case thrust washer (12) as determined by the selective thrust washer check to the oil pump. Retain with J 36850 or equivalent.
2. Install J 38588-1 .
3. Install the oil pump to case gasket (11) onto the pump. Retain with J 36850 or equivalent.
4. Install the converter housing and the oil pump assembly.
5. Remove J 38588-1 .

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

Important: Be sure converter housing is aligned evenly with the case before installing bolts.

6. Install the converter housing to case bolts (4).

Tighten
Tighten the bolts to 40 N·m (29 lb ft) in an alternating pattern.

7. Rotate the oil pump drive gear using J 23082-A to check for free movement.