For 1990-2009 cars

#### Tools Required

J 42960-1 Fuel Tank Drain Hose

### Removal Procedure

Caution: Gasoline or gasoline vapors are highly flammable. A fire could occur if an ignition source is present. Never drain or store gasoline or diesel fuel in an open container, due to the possibility of fire or explosion. Have a dry chemical (Class B) fire extinguisher nearby.

1. Relieve the fuel system pressure. Refer to Fuel Pressure Relief .
2. Remove the filler cap.
3. Insert the J 42960-1 into the fuel tank.
4. Position an approved drain container near the vehicle.
5. Use an air operated pump to drain the tank into an approved container.