For 1990-2009 cars

1. Disconnect the wire harness connectors from the electrical components.

Important: Excessive force on the case pass through connector may damage the connector.

2. Remove the wire harness assembly (80). If the wire harness assembly does not need servicing, it is not necessary to remove it from the case.
3. Remove the main case electrical connector (55) from the case, if necessary.