For 1990-2009 cars

### Removal Procedure

1. Set the parking brake.
2. Move the gear selector to the full rear position (1st gear).
3. Remove the I/P bezel. Refer to Instrument Panel Accessory Trim Plate Replacement in Instrument Panel, Gauges and Console.
4. Remove the radio (2) mounting screws (1).
5. Remove the radio (2) from the HVAC control head mounting bracket (1).
6. Disconnect the antenna connector (1).
7. Disconnect the wiring harness connector (2).

### Installation Procedure

1. Connect the wiring harness connector (2).
2. Connect the antenna connector (1).
3. Install the radio (2) into the HVAC control head mounting bracket (1).
4. Install the radio mounting screws (1) until fully seated and not stripped.
5. Install the I/P bezel. Refer to Instrument Panel Accessory Trim Plate Replacement in Instrument Panel, Gauges and Console.
6. Install the scan tool.
7. Select RADIO THEFT from the SPECIAL FUNCTIONS menu.
8. Follow the instructions on the screen.