For 1990-2009 cars

### Circuit Description

This diagnostic trouble code (DTC) can set if there is an engine torque limitation caused by the traction control system, the transmission, or an engine speed limitation.

### Conditions for Running the DTC

The engine speed is more than 40 RPM.

### Conditions for Setting the DTC

The engine output torque exceeds a certain value for 600 seconds.

### Action Taken When the DTC Sets

• | The control module illuminates the malfunction indicator lamp (MIL) on the second consecutive ignition cycle that the diagnostic runs and fails.

• | The control module records the operating conditions at the time the diagnostic fails. The first time the diagnostic fails, the control module stores this information in the Failure Records. If the diagnostic reports a failure on the second consecutive ignition cycle, the control module records the operating conditions at the time of the failure. The control module writes the operating conditions to the Freeze Frame and updates the Failure Records.

### Conditions for Clearing the MIL/DTC

• | The control module turns OFF the malfunction indicator lamp (MIL) after 3 consecutive ignition cycles that the diagnostic runs and does not fail.

• | A current DTC, Last Test Failed, clears when the diagnostic runs and passes.

• | A history DTC clears after 40 consecutive warm-up cycles, if no failures are reported by this or any other emission related diagnostic.

• | Clear the MIL and the DTC with a scan tool.

#### DTC P1845 Torque Limit Management

Step | Action | Yes | No
--- | --- | --- | ---
Schematic Reference: Engine Controls Schematics
1 | Did you perform the Diagnostic System Check-Engine Controls? | Go to Step 2 | Go to Diagnostic System Check - Engine Controls
2 | Are any other DTCs set? | Go to Diagnostic Trouble Code (DTC) List | Go to Step 3
3 | Important:

• | Perform the idle learn procedure when replacing the ECM or the throttle body.

• | This vehicle is equipped with a theft deterrent system which interfaces with the engine control module (ECM). Program the new ECM with the frequency code of the theft deterrent module that is currently on the vehicle.

Replace the ECM. Refer to Engine Control Module Replacement .

Did you complete the action?

Go to Step 4

--

4 |

1. Use the scan tool in order to clear the DTCs.
2. Turn OFF the ignition for 30 seconds.
3. Start the engine.
4. Operate the vehicle within the Conditions for Running the DTC as specified in the supporting text.

Does the DTC run and pass?

Go to Step 5

--

5 | With a scan tool, observe the stored information, Capture Info. Does the scan tool display any DTCs that you have not diagnosed? | Go to Diagnostic Trouble Code (DTC) List | System OK