For 1990-2009 cars

### Removal Procedure

1. Remove the LH front seat. Refer to Seat Replacement in Seats.
2. Remove the front carpeting and insulation. Refer to Front Floor Panel Carpet Replacement in Interior Trim.
3. Remove the rear floor air outlet nut.
4. Remove the rear floor air outlet.

### Installation Procedure

1. Install the rear floor air outlet.
2. Install the rear floor air outlet nut.
3. Install the front carpeting and insulation. Refer to Front Floor Panel Carpet Replacement in Interior Trim.
4. Install the LH front seat. Refer to Seat Replacement in Seats.