For 1990-2009 cars

### Replacement Procedure

1. Remove the cigarette lighter.

1.1. | Remove the ashtray. Refer to Ashtray Replacement .

1.2. | Remove the cigarette lighter from the ashtray with small flat-bladed tools.

1.3. | Remove the wiring connector from the lighter.

2. Install the cigarette lighter.

2.1. | Install the wiring connector to the lighter.

2.2. | Install the cigarette lighter to ashtray by firmly seating.

2.3. | Install the ashtray. Refer to Ashtray Replacement