For 1990-2009 cars

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the tire and the wheel. Refer to Tire and Wheel Removal and Installation in Tires and Wheels.
3. Remove the brake caliper. Refer to Front Brake Caliper Replacement .
4. Remove front brake caliper bracket bolts (1) and discard.
5. Remove the front brake caliper bracket from the steering knuckle.

### Installation Procedure

1. Ensure the front brake caliper bracket mounting surfaces (1) are clean.
2. Chase the caliper bracket mounting threads in the steering knuckle to remove any residual locking compound.
3. Install the caliper bracket to the steering knuckle.
4. Coat the new caliper bracket bolts (1) with 272 Threadlocker, GM P/N 12345493 or equivalent.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

5. Install the new caliper bracket bolts (1).

Tighten
Tighten the caliper bracket bolts (1) to 95 N·m (70 lb ft) on the first pass and additional 37 degrees on the second pass.

6. Install the brake caliper. Refer to Front Brake Caliper Replacement .
7. Install the tire and wheel assembly. Refer to Tire and Wheel Removal and Installation in Tires and Wheels.
8. Lower the vehicle.
9. Fill the master cylinder reservoir.