For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the compressor. Refer to Air Compressor Replacement .
3. Unclip the tube (1) from the vehicle body.
4. Remove the filter from the tube (1).

### Installation Procedure

1. Install the filter to the tube (1).
2. Clip the tube (1) to the vehicle body.
3. Install the compressor. Refer to Air Compressor Replacement .
4. Lower the vehicle.