For 1990-2009 cars

### Removal Procedure

1. Remove the door trim panel. Refer to Rear Side Door Trim Panel Replacement in Doors.
2. Remove the radio rear side door speaker screws (1).
3. Disconnect the speaker connector.

### Installation Procedure

1. Connect the speaker connector.
2. Install the speaker screws (1) until fully seated and not stripped.
3. Install the door trim panel. Refer to Rear Side Door Trim Panel Replacement in Doors.