For 1990-2009 cars

### Removal Procedure

1. Remove the front seat. Refer to Seat Replacement .
2. Remove the front seat back panel. Refer to Driver Seat and Passenger Seat Back Cushion Finish Panel Replacement .
3. Remove the front seat back inner liner. The front seat back inner liner unhooks from upper and lower corners. Use a small thin-bladed tool to assist with releasing of lower hooks.

### Installation Procedure

1. Install the front seat back inner liner. Install the front seat back inner liner hooks to upper and lower corners. Use a small thin-bladed tool to assist with engaging of lower hooks.
2. Install the front seat back panel. Refer to Driver Seat and Passenger Seat Back Cushion Finish Panel Replacement .
3. Install the front seat. Refer to Seat Replacement .