For 1990-2009 cars

• | The flexible hydraulic brake hoses transmit hydraulic pressure from the brake pipes to the front and rear brake calipers. Inspect the flexible hydraulic brake hoses at least twice a year. The vehicle must be on a lift to perform the inspection.

• | Use a light and a mirror to inspect the hoses for the following conditions:

- | Inspect for road hazard damage. Replace the brake hose(s) if road hazard damage is evident.

- | Inspect for cracks. Replace the brake hose(s) if a crack(s) is evident.

- | Inspect for leaks. Replace the brake hose(s) if a leak(s) is evident.

- | Inspect for blisters Replace the brake hose(s) if a blister(s) is evident.

- | Inspect for chafing. Replace the brake hose(s) if chafing if evident.