For 1990-2009 cars

### Removal Procedure

1. Remove the mirror lens. Refer to Outside Rearview Mirror Glass Replacement .
2. Disconnect the mirror motor electrical connector.
3. Remove the mirror motor screws.
4. Remove the mirror motor.

### Installation Procedure

1. Position the mirror motor to the mirror housing.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the mirror motor screws.

Tighten
Tighten the mirror motor screws to 10 N·m (89 lb in).

3. Connect the mirror motor electrical connector.
4. Install the mirror lens. Refer to Outside Rearview Mirror Glass Replacement .