For 1990-2009 cars

### Removal Procedure

1. Use screwdrivers to carefully lever the door courtesy lamp from the door and remove the door courtesy lamp.
2. Remove the metal protective cover from the back side of the door courtesy lamp (1).
3. Remove the bulb.

### Installation Procedure

1. Install the bulb.
2. Install the metal protective cover to the back of the door courtesy lamp.
3. Snap the door courtesy lamp in place to install (1).