For 1990-2009 cars

### Removal Procedure

Important: The switch panel will pop out with gently prying action.

1. Remove the rear heated seat switch panel from front floor console rear housing.
2. Remove the connector to switch.
3. Remove the rear heated seat switch from panel.

### Installation Procedure

1. Install the rear heated seat switch to panel.
2. Install the connector to switch.
3. Install the rear heated switch panel to front floor console vent housing.