For 1990-2009 cars

### Removal Procedure

With a small flat-bladed tool pry on the side of the fuel door switch and remove from the instrument panel (IP) accessory trim plate.

This will disengage the fuel door switch from the electrical connector.

### Installation Procedure

1. Align the fuel door switch with the electrical connector in the IP accessory trim plate.
2. Push inward on the fuel door switch until fully seated in the IP accessory trim plate.

This will engage the electrical connector to the fuel door switch.