For 1990-2009 cars

### Schedule II - Long Trip/Highway Service

Follow this schedule if none of the conditions listed under Schedule I apply. This engine is designed to operate up to 10,000 miles (16 000 km) between oil changes. The oil will be contaminated much sooner if the engine is not frequently operated under normal operating temperatures.

What to Service | When to Perform
--- | ---
Engine Oil and Filter Replacement | First 5,000 miles (8 000 km) or every 3 months, then every 10,000 miles (16 000 km) or 12 months
Tire Rotation and Brake System Inspection | First 5,000 miles (8 000 km), then every 10,000 miles (16 000 km)
Air Cleaner Filter Inspection | Every 15,000 miles (24 000 km)
Passenger Compartment Air Filter (Pollen Filter) Replacement | Every 15,000 miles (24 000 km)
Air Cleaner Filter Replacement | Every 30,000 miles (48 000 km)
Fuel Tank, Cap and Lines Inspection | Every 30,000 miles (48 000 km)
Rear Axle Fluid Level Check | Every 30,000 miles (48 000 km)
Engine Accessory Drive Belt Inspection | Every 60,000 miles (96 000 km)
Spark Plug Replacement | Every 100,000 miles (160 000 km)
Spark Plug Wire Inspection | Every 100,000 miles (160 000 km)
Camshaft Drive Belt Replacement | Refer to Explanation of Scheduled Services.
Fuel Filter Replacement | Every 100,000 miles (160 000 km)
Engine Coolant Replacement | Every 150,000 miles (240 000 km)