For 1990-2009 cars

### Removal Procedure

1. Disable the SIR system. Refer to Disabling the SIR System .
2. Remove the front door trim panel. Refer to Front Side Door Trim Panel Replacement .
3. Remove the front door water deflector. Refer to Front Side Door Water Deflector Replacement .
4. Disconnect the inflatable restraint side impact sensor electrical connector.
5. Remove the five rivets by drilling out.
6. Remove the mounting plate from the door.

### Installation Procedure

1. Install the mounting plate to door.
2. Install the new rivets to mounting plate and door.
3. Connect the inflatable restraint side impact sensor electrical connector.
4. Install the front door water deflector. Refer to Front Side Door Water Deflector Replacement .
5. Install the front door trim panel. Refer to Front Side Door Trim Panel Replacement .
6. Enable the SIR system. Refer to Enabling the SIR System in Restraints.