For 1990-2009 cars

Step | Action | Values | Yes | No
--- | --- | --- | --- | ---
Definition: Windshield washer solvent level indicator is inoperative.
1 | Did you perform the Instrument Cluster System Check? | -- | Go to Step 2 | Go to Instrument Cluster System Check
2 | Disconnect the windshield washer solvent level switch connector. Is the indicator lamp ON? | -- | Go to Step 4 | Go to Step 3
3 |

1. Test for a short to ground in circuit XB3.
2. IF OK replace the gauge cluster.

Is the repair or replacement complete?

--

Go to Step 5

--

4 | Replace the windshield washer solvent level switch. Is the replacement complete? | -- | Go to Step 5 | --
5 |

1. Connect all connectors and components that were removed in previous steps.
2. Verify that the low windshield washer solvent level indicator operates properly.

Does the low windshield washer solvent level indicator operate properly?

--

System OK

Go to Step 2