For 1990-2009 cars

### Removal Procedure

1. Raise the hood.
2. Back off the primary hood latch/pilot pin lock nut.
3. Thread the pin out of the hood.

### Installation Procedure

1. Thread the pin into the hood.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Adjust the hood flush clearances. Refer to Vertical Hood Adjustment .

Tighten
Tighten the primary hood latch/pivot pin lock nut to 40 N·m (30 lb ft).

3. Lower the hood.