For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Body Control Module (BCM) | Mounted on the RH A-pillar, behind the trim panel | Body Control System Component Views in Body Control System | Body Control System Connector End Views in Body Control System
Data Link Connector (DLC) | Attached to the I/P carrier, to the left of the steering column | -- | Data Link Communications Connector End Views in Data Link Communications
Electronic Brake/Traction Control Module (EBTCM) | LH front of the engine compartment, mounted to the lower rail | Antilock Brake System Component Views in Antilock Brake System | Antilock Brake System Connector End Views in Antilock Brake System
Engine Control Module (ECM) | LH front of the engine compartment, in the ECM housing | Engine Controls Component Views in Engine Controls | Engine Controls Connector End Views in Engine Controls
Engine Coolant Temperature Gauge Sensor | Mounted in the coolant bridge | Engine Controls Component Views in Engine Controls | Engine Controls Connector End Views in Engine Controls
Engine Oil Level Sensor | Lower RH front of the engine block | -- | --
Engine Oil Pressure Gauge Switch | Lower RH front of the engine block | -- | --
Front Disc Brake Pad Wear Sensor (LH) | Attached to the LH front brake caliper | Instrument Panel, Gages, and Console Component Views | --
Front Disc Brake Pad Wear Sensor (RH) | Attached to the RH front brake caliper | Instrument Panel, Gages, and Console Component Views | --
Fuel Sender | Underneath the rear of the vehicle, inside the fuel tank | -- | --
Fuel Sensor | Part of the fuel sender | -- | --
Fuse Block | Mounted to the I/P, lower LH side of the steering column | -- | --
Gauge Cluster | LH side of the I/P, just to the left and above the heater and A/C control | -- | Instrument Panel, Gages, and Console Connector End Views
Instrument Cluster | LH side of the I/P, above the steering column | -- | Instrument Panel, Gages, and Console Connector End Views
Multifunction Relay K134 | Under the LH side of the I/P | Instrument Panel, Gages, and Console Component Views | Lighting Systems Connector End Views in Lighting Systems
C102 (brown connector) | I/P wiring harness to engine wiring harness, in the LH front of the engine compartment, just behind the battery | Wiper/Washer Component Views in Wipers/Washer System | Inline Harness Connector End Views in Wiring Systems
C105 (white connector) | I/P wiring harness to ECM wiring harness, in the LH front of the engine compartment, just behind the battery | Wiper/Washer Component Views in Wipers/Washer System | Inline Harness Connector End Views in Wiring Systems
C115 | ECM wiring harness to the engine coolant temperature jumper harness, at rear center of the engine, below C112 | -- | Inline Harness Connector End Views in Wiring Systems
C200A | I/P wiring harness to body wiring harness, at lower LH A-pillar | Power and Grounding Component Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C200B | I/P wiring harness to body wiring harness, at lower LH A-pillar | Power and Grounding Component Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C400 | Body wiring harness to fuel sender wiring harness, beneath the vehicle, near the front of the fuel tank | -- | Inline Harness Connector End Views in Wiring Systems
G103 | Body and I/P wiring harnesses, located at the LH front of the engine compartment, underneath the battery tray | Wiper/Washer Component Views in Wipers/Washer System | --
G400 | Body wiring harness, in the lower LH corner of the rear compartment, near the LH stop/taillamp | -- | --
P103 | Lower LH A-pillar, forward of G200 | Power and Grounding Component Views in Wiring Systems | --
P104 | LH engine compartment, at the front of the ECM housing | -- | --
P110 | Rear LH corner of the engine compartment | -- | --
S200 | I/P wiring harness, approximately 14 cm (7 in) from P110, towards connector C200 branch break off | -- | --
S204 | I/P wiring harness, approximately 16 cm (6 in) from P110, towards connector C200 branch break off | -- | --
S215 | I/P wiring harness, approximately 18 cm (7 in) from cruise release switch and stoplamp switch branch break off, to the right of the DLC connector branch break off | -- | --
S222 | I/P wiring harness, approximately 33 cm (13 in) from cruise release switch and stoplamp switch branch break off, near G201 branch break off | -- | --
S228 | I/P wiring harness, approximately 8 cm (3 in) from cruise release switch and stoplamp switch branch break off, to the left of the DLC connector branch break off | -- | --
S229 | I/P wiring harness, approximately 20 cm (8 in) from cruise release switch and stoplamp switch branch break off, to the right of the DLC connector branch break off | -- | --
S238 | I/P wiring harness, approximately 18 cm (7 in) from cruise release switch and stoplamp switch branch break off, to the right of the DLC connector branch break off | -- | --
S248 | I/P wiring harness, mounted in harness channel behind LH side of heater and A/C control, approximately 5 cm (2 in) from gauge cluster connector branch break off | -- | --
S251 | I/P wiring harness, approximately 18 cm (7 in) from cruise release switch and stoplamp switch branch break off, to the right of the DLC connector branch break off | -- | --
S252 | I/P wiring harness, approximately 14 cm (7 in) from P110, before the power steering control module and multifunction relay (K134) branch break offs | -- | --
S262 | I/P wiring harness, approximately 9 cm (4 in) from cruise release switch and stoplamp switch branch break off, to the left of the DLC connector branch break off | -- | --
S267 | Body wiring harness, approximately 23 cm (9 in) from C200, in cross-car portion of body harness center console area | -- | --
S400 | Body wiring harness, approximately 15 cm (6 in) from G400 branch break off, towards C401 branch break off | -- | --