For 1990-2009 cars

### Removal Procedure

1. Press the rear section of the sidemarker lamp inward and slide rearward.
2. Remove the front sidemarker lamp from the front bumper fascia.
3. Disconnect the electrical connector from the side marker lamp.
4. Remove the side marker lamp bulb/socket by rotating counterclockwise.
5. Remove the side marker lamp bulb from the socket .

### Installation Procedure

1. Install the side marker lamp bulb to the socket.
2. Install the side marker lamp bulb/socket to the sidemarker lamp by rotating clockwise.
3. Connect the electrical connector to the side marker lamp.
4. Insert the pivot tab end of the front sidemarker lamp into the front fascia, pressing until fully seated.