For 1990-2009 cars

### Removal Procedure

1. Remove the grille. Refer to Grille Replacement in Exterior Trim.
2. Disconnect the pump wiring harness connector (8).
3. Remove the motor (7) from the solvent container (5).
4. Remove the filter (6).
5. Inspect the filter. Clean or replace as needed.

### Installation Procedure

1. Install the filter (6).
2. Install the motor (7) to the solvent container (5).
3. Connect the pump connector (8).
4. Install the grille. Refer to Grille Replacement in Exterior Trim.
5. Verify the motor operation.