For 1990-2009 cars

## Speaker Grille Replacement Front Door

### Removal Procedure

1. Disable the SIR system, if equipped with the inflatable restraint side impact system. Refer to Disabling the SIR System in Restraints.
2. Remove the trim panel. Refer to Front Side Door Trim Panel Replacement .
3. Remove the speaker grille clips.
4. Remove the speaker grille.

### Installation Procedure

1. Install the speaker grille.
2. Install the speaker grille clips.
3. Install the trim panel. Refer to Front Side Door Trim Panel Replacement .
4. Enable the SIR system, if equipped with the inflatable restraint side impact system. Refer to Enabling the SIR System in Restraints.

## Speaker Grille Replacement Rear Door

### Removal Procedure

1. Remove the trim panel. Refer to Rear Side Door Trim Panel Replacement .
2. Pull up on the clips in order to remove the speaker grille.

### Installation Procedure

1. Push on the clips in order to install the grille.
2. Install the trim panel. Refer to Rear Side Door Trim Panel Replacement .