For 1990-2009 cars

Take note of the following statements:

• | Do not try to repair a damaged energy absorber.

• | Replace the energy absorber if damaged.

• | Do not apply heat to the energy absorbers.

• | Do not weld the energy absorbers.

Look at the following components for signs of visible distortion:

• | Look at the bumper impact bar bracket.

• | Look at the piston tube. Scuffing of the piston tube occurs when it is stroked and this is considered to be normal.

• | Look at the frame bracket.

• | Look at the cylinder tube.

Replace the energy absorber if obvious damage is evident. Replace the energy absorber if a collision is so severe that the bumper impact bar does not return to its original position.