For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 | Turn the headlamp switch to the PARK position. | All exterior lamps turn ON. | Exterior Lamps Inoperative
2 | Turn the headlamp switch to the PARK position. | The front side marker lamps and the rear side marker lamps turn ON. |

• | Side Marker Lamps Inoperative

• | Side Marker Lamps Inoperative

3 | Turn the headlamp switch to the PARK position. | The park lamps and the taillamps turn ON. |

• | Park Lamps Inoperative - Front

• | Tail Lamps Inoperative

4 | Turn the headlamp switch to the PARK position. | The rear license lamps and the middle taillamp turn ON. | License and Tail Lamps Inoperative
5 | Press the brake pedal. | The stop lamps and the auxiliary brake lamp turn ON. | Stop Lamps Inoperative - One
6 |

1. Engage the turn signal switch in order to turn ON the left side turn indicator.
2. Engage the turn signal switch in order to turn ON the right side indicator.

• | The left indicator and the right indicator operate properly.

• | The left cornering lamp and the right cornering lamp operate properly.

• | Turn Signal Indicators Inoperative

• | Cornering Lamps Inoperative

7 |

1. Engage the turn signal switch in order to turn ON the left side turn indicator.
2. Engage the turn signal switch in order to turn ON the right side indicator.

The left turn signal lamp and the right signal lamp operate properly.

• | Turn Signal Lamps Inoperative

• | Turn Signal Lamps Inoperative

8 | Press the hazard warning switch. | The warning lamps operate properly. | Hazard Lamps Inoperative
* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.