For 1990-2009 cars

### Winter Mode Switch

#### Removal Procedure

1. Remove the gear selector boot from the console.

The boot snaps into console and can be removed by gently pulling on front end of boot.

2. Remove the connector from switch.

Important: Do not pry the switch from console as damage to console trim panel may occur.

Dislodge the switch from console by reaching under console opening near gear selector.

### Installation Procedure

1. Install the connector to the switch.
2. Install the switch to the console making sure to fully seat.
3. Install the gear selector boot to the console by snapping into place.

### Shift Indicator

#### Removal Procedure

1. Remove the gear selector boot from console.

The boot snaps into the console and can be removed by gently pulling on the front end of the boot.

Important: Do not pry the indicator from console as damage to console trim may occur.

2. Dislodge the indicator from the console by reaching under the console opening near the gear selector.
3. Remove the connector from the indicator.
4. Remove the indicator.

### Installation Procedure

1. Install the connector to the shift indicator.
2. Install the shift indicator to the console making sure to fully seat.
3. Install the gear selector boot to console by snapping into place.

### Power Window Switch

#### Removal Procedure

1. Remove the gear selector boot from console.

The boot snaps into console and can be removed by gently pulling on front end of boot.

2. Remove the connector from power window switch.
3. Dislodge the switch from console by reaching under console opening near gear selector.

Important: Do not the switch from console as damage to console trim panel may occur.

### Installation Procedure

1. Install the switch into the console by firmly seating.
2. Install the connector to the switch.
3. Install the gear selector boot to the console by snapping into place.