For 1990-2009 cars

### Removal Procedure

1. Remove the front seat. Refer to Seat Replacement .
2. Remove the front seatback panel. Refer to Driver Seat and Passenger Seat Back Cushion Finish Panel Replacement .
3. Remove the front seatback inner liner.

The front seatback inner liner unhooks from the upper and lower corners. Use a small thin-bladed tool in order to assist with releasing the lower hooks.

### Installation Procedure

1. Install the front seatback inner liner.

Install the hooks to the front seatback inner liner at the upper and lower corners. Use a small thin-bladed tool in order to assist engaging the lower hooks.

2. Install the front seatback panel. Refer to Driver Seat and Passenger Seat Back Cushion Finish Panel Replacement .
3. Install the front seat. Refer to Seat Replacement .