For 1990-2009 cars

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the rear exhaust section. Refer to Resonator Replacement .
3. Remove the heat shield nuts.
4. Remove the heat shield.

### Installation Procedure

1. Install the heat shield.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the heat shield nuts to the heat shield.

Tighten
Tighten the heat shield nuts to 2 N·m (18 lb in).

3. Install the rear exhaust section. Refer to Resonator Replacement .
4. Inspect all exhaust system clearances. Refer to Exhaust System Clearances .
5. Lower the vehicle.