For 1990-2009 cars

1. Remove the oil seal rings (32).
2. Inspect the oil seal ring grooves for wear and damage.
3. Remove the overrun lockout valve plug retainer plate (702).
4. Remove the lockout valve plug (703).
5. Remove the overrun lockout valve spring (704).
6. Remove the overrun lockout valve (705).
7. Inspect the overrun lockout valve for:

• | nicks

• | burrs

• | scoring

8. Remove the reverse lockout control valve plug retainer plate (702).
9. Remove the reverse lockout control valve plug (703).
10. Remove the reverse lockout control valve spring (704).
11. Remove the reverse lockout control valve (706).
12. Inspect the reverse lockout control valve for:

• | nicks

• | burrs

• | scoring