For 1990-2009 cars

### Removal Procedure

1. Lower the window to the bottom of the door.
2. Remove the trim panel. Refer to Rear Side Door Trim Panel Replacement .
3. Lift up on the rear edge of the inner belt sealing strip in order to remove.

### Installation Procedure

1. Install the sealing strip:

• | Start at the rear edge.

• | Press firmly onto the flange.

• | Seat the strip using a rubber mallet.

2. Install the trim panel. Refer to Rear Side Door Trim Panel Replacement .
3. Raise the window.